# GetRawJoystickRZ

## Description

Returns the current rotational Z value (if applicable) for the physical joystick at the given index. This will be in the range -1.0 to 1.0 with 0 being centered. In reality some joystick devices use this value for a second analogue stick.

## Definition

float GetRawJoystickRZ( index )

float agk::GetRawJoystickRZ( UINT index )

## Parameters

- index - The ID of the joystick to check.