# GetRawGyroVelocityY

## Description

If a gyroscope exists, returns the Y component of the current device rotation speed. If you have not used SetOrientationAllowed to select your desired orientation then this command will lock the device in the current orientation to prevent the screen from rotating. You should use SetOrientationAllowed if you want to enable screen rotation when using the gyroscope.

## Definition

float GetRawGyroVelocityY()

float agk::GetRawGyroVelocityY()