SET BSP CAMERA COLLISION RADIUS This command will set the BSP camera collision radius used during collision detection.
Syntax
    SET BSP CAMERA COLLISION RADIUS Collision Index, Camera Number, X, Y, Z
Parameters
    Collision Index
Integer This value is an integer number such as 1.
    Camera Number
Integer Specify a camera number between 0 and 32.
    X
Float Specify the X position value.
    Y
Float Specify the Y position value.
    Z
Float Specify the Z position value.
Returns
This command does not return a value.
Description
You can use this command in combination with the SET BSP COLLISION HEIGHT ADJUSTMENT to fine tune your collision entity within the BSP universe.
Example Code

    No example code is provided for this command
See also
WORLD Commands Menu Index