CONTROL CAMERA USING ARROWKEYS This command will monitor the arrow keys and move the camera based on their activity.
Syntax
    CONTROL CAMERA USING ARROWKEYS Camera Number, MoveSpeed, TurnSpeed
Parameters
    Camera Number
Integer The camera number
    MoveSpeed
Float The move value
    TurnSpeed
Float The turn value
Returns
This command does not return a value.
Description
The up and down arrow keys move the camera forward and backward. The left and right arrow keys turn the camera left and right respectively.
Example Code
    autocam on:backdrop on

    make matrix 1,4000,4000,100,100

    set matrix height 1,50,50,500

    update matrix 1

    position camera 0,0,500,500

    point camera 0,2000,0,2000

    make camera 1

    position camera 1,0,500,500

    point camera 1,2000,0,2000

    set camera view 1,10,10,100,100

    while mouseclick()<>1

    if inkey$()="z" then set current camera 0 : c=0

    if inkey$()="x" then set current camera 1 : c=1

    control camera using arrowkeys c,1,1

    endwhile

    while mouseclick()=1 : endwhile

    delete matrix 1:autocam off:backdrop off

    end
See also
CAMERA Commands Menu Index