SET NET CONNECTION This command will set the machine to a specific connection.
Syntax
    SET NET CONNECTION Connection Number
    SET NET CONNECTION Connection Number,Address Data
Parameters
    Connection Number
Integer The Connection Number can be obtained by using the index of the checklist produced by the PERFORM CHECKLIST FOR NET CONNECTIONS command
    Address Data
String If you connect by TCP/IP the Address Data should be an IP and Url Address. If the connection type is MODEM, you should specify a phone number if you are dialling or leave blank if you are answering
Returns
This command does not return a value.
Description
The Connection Number can be obtained by using the index of the checklist produced by the PERFORM CHECKLIST FOR NET CONNECTIONS command. You can optionally specify Address Data depending on the connection type. If you connect by TCP/IP the Address Data should be an IP and Url Address. If the connection type is MODEM, you should specify a phone number if you are dialling or leave blank if you are answering. If the connection type is SERIAL, it is recommended you leave the Address Data blank to obtain the Windows Serial Configuration Dialogue Box. IPX connections require no additional Address Data.
Example Code
    perform checklist for net connections

    cls

    print "CONNECTIONS (Can Occur In Any Order)"

    for c=1 to checklist quantity()

    print c;". ";checklist string$(c)

    next c

    SelectionIndex=0

    if checklist quantity()<>0

    while SelectionIndex<1 or SelectionIndex>checklist quantity()

    print  : input "Select A Number>";SelectionIndex

    endwhile

    set net connection SelectionIndex,( IP Address or PhoneNumber )

    endif
See also
MULTIPLAYER Commands Menu Index