PHY MAKE PULLEY JOINT ratio
Syntax
    PHY MAKE PULLEY JOINT ID, A, B, x1#, y1#, z1#, x2#, y2#, z2#, x3#, y3#, z3#, x4#, y4#, z4#, distance#, stiffness#, value#
    PHY MAKE PULLEY JOINT ID, A, B
Parameters
    ID
Integer identification number of the joint, joint ID numbers are unique
    A
Integer the first rigid body object to be attached to the joint
    B
Integer the second rigid body object to be attached to the joint
    x1#
Float position
    y1#
Float position
    z1#
Float position
    x2#
Float position
    y2#
Float position
    z2#
Float position
    x3#
Float position
    y3#
Float position
    z3#
Float position
    x4#
Float position
    y4#
Float position
    z4#
Float position
    distance#
Float distance
    stiffness#
Float stiffness
    value#
Float This value is a float number such as 0.5
Returns
Example Code

    No example code is provided for this command