PHY SET 6DOF JOINT GEAR Apply gearing to the angular motion e.
Syntax
    PHY SET 6DOF JOINT GEAR ID, state
Parameters
    ID
Integer identification number of the joint
    state
Integer a value of 1 will enable gearing whereas a value of 0 will disable it
Returns
Description
g. body 2s angular motion is twice that of body 1s etc. This is a property to control the general behaviour of a 6DOF joint and is used to enable or disable gearing.
Example Code

    No example code is provided for this command