POSITION CAMERA This command will set the position of the camera in 3D space.
Syntax
    POSITION CAMERA X, Y, Z
    POSITION CAMERA Camera Number, X, Y, Z
    POSITION CAMERA Camera Number, Vector
Parameters
    Camera Number
Integer The camera number
    X
Float The x position in 3d
    Y
Float The y position in 3d
    Z
Float The z position in 3d
Returns
This command does not return a value.
Description
The coordinates should be real numbers.
Example Code
    autocam on

    make matrix 1,4000,4000,100,100

    set matrix height 1,50,50,500

    update matrix 1

    set camera rotation xyz 0

    position camera 0,0,100,-500

    while mouseclick()<>1

    x#=cos(a#)*500 : z#=sin(a#)*500

    a#=a#+1.0 : if a#>359 then a#=a#-360

    position camera 0,x#,100,z#

    point camera 0,500,0,500

    endwhile

    while mouseclick()=1:endwhile

    delete matrix 1:autocam off

    end
See also
CAMERA Commands Menu Index