SET BSP CAMERA COLLISION This command will set the collision sphere of the camera for the BSP world.
Syntax
    SET BSP CAMERA COLLISION Collision Index, Camera Number, Radius, Response
Parameters
    Collision Index
Integer This value is an integer number such as 1.
    Camera Number
Integer Specify a camera number between 0 and 32.
    Radius
Float This value is a float number such as 0.5
    Response
Integer This value is an integer number such as 1.
Returns
This command does not return a value.
Description
This will automatically adjust the position of the camera when it attempts to enter solid BSP geometry. The camera will be repositioned to produce the smoothest collision response. If the Response value is set to one, the new position backtracks to the last collision free position when a hit occurs. It is worth noting that even commands that reposition the camera are subject to the BSP collision once active. To avoid problems repositioning the camera, simply deactivate and reactivate the collision during positioning.
Example Code

    No example code is provided for this command
See also
WORLD Commands Menu Index