LFX GET LIGHT COLOR I This command gets the current component intensity value of the specified light belonging to the device.
Syntax
    Return Integer=LFX GET LIGHT COLOR I(Device Number, Light Number)
Parameters
    Device Number
Integer Specifies the device number to read from
    Light Number
Integer Specifies the light number belonging to the device
Returns
An intensity component in the range of 0 to 255
Example Code

    No example code is provided for this command
See also
LIGHTFX9 Commands Menu Index