PHY SET RIGID BODY KINEMATIC ROTATION Set the position of the specified kinematic rigid body.
Syntax
    PHY SET RIGID BODY KINEMATIC ROTATION ID, x#, y#, z#
Parameters
    ID
Integer ID number of the rigid body
    x#
Float angle of rotation on X axis
    y#
Float angle of rotation on Y axis
    z#
Float angle of rotation on Z axis
Returns
Example Code

    No example code is provided for this command