SC_ErrorMode
SYNTAX
SC_ErrorMode mode
-mode: the error mode to use from this point onwards.
0=ignore errors
1=report errors and continue
2=report errors and quit (default)
Sets the error mode to use for all collision commands after this point. Ignoring errors can cause
the collision system to behave unexpectedly as any failed setups/updates/deletes will not be reported.
Can be called as many times as needed during the running of the system.
RELATED INFO
Collision Commands Menu
Index