JOYSTICK X This command will return the X axis value of the default analogue joystick.
Syntax
    Return Integer=JOYSTICK X()
Returns
The command will return the x axis value of the default analogue joystick
Example Code
    do

    cls

    print "joystick x "+str$(joystick x())

    print "joystick y "+str$(joystick y())

    print "joystick z "+str$(joystick z())

    loop

    end
See also
INPUT Commands Menu Index