ROLL CAMERA LEFT This command will roll the camera left.
Syntax
    ROLL CAMERA LEFT Angle Value
    ROLL CAMERA LEFT Camera Number, Angle Value
Parameters
    Camera Number
Integer The camera number
    Angle Value
Float The value of the angle can be positive or negative
Returns
This command does not return a value.
Description
The rotation is independent of any axis orientation and allows free motion. The value of the angle can be positive or negative. The angle must be specified using a real value.
Example Code
    autocam on

    make matrix 1,4000,4000,100,100

    set matrix height 1,50,50,500

    update matrix 1

    while mouseclick()<>1

    set cursor 0,0

    print "USE ARROW KEYS TO ROTATE / A+Z Roll Camera"

    if upkey()=1 then pitch camera up 0,1

    if downkey()=1 then pitch camera down 0,1

    if leftkey()=1 then turn camera left 0,1

    if rightkey()=1 then turn camera right 0,1

    if inkey$()="a" then roll camera left 0,1

    if inkey$()="z" then roll camera right 0,1

    endwhile

    while mouseclick()=1 : endwhile

    delete matrix 1:autocam off

    end
See also
CAMERA Commands Menu Index