ROTATE LISTENER This command will set the direction of the listener.
Syntax
    ROTATE LISTENER X,Y,Z
Parameters
    X
Float The x position
    Y
Float The y position
    Z
Float The z position
Returns
This command does not return a value.
Description
The 3D sounds being played would sound different based on which direction the listener was facing.
Example Code
    cls

    load sound "man.wav",1

    play sound 1

    rotate listener 100,100,500

    wait 1000*8

    rotate listener 100,100,-500

    wait 1000*8

    stop sound 1

    do

    loop

    end
See also
SOUND Commands Menu Index