PHY SET 6DOF JOINT DRIVE ANGULAR VELOCITY Set the drive angular velocity.
Syntax
    PHY SET 6DOF JOINT DRIVE ANGULAR VELOCITY ID, x#, x#, z#
Parameters
    ID
Integer identification number of the joint
    x#
Float angular velocity on the X axis
    x#
Float angular velocity on the X axis
    z#
Float angular velocity on the Z axis
Returns
Example Code

    No example code is provided for this command