PHY SET 6DOF JOINT MOTION Z Set the range of motions allowed on the Z axis.
Syntax
    PHY SET 6DOF JOINT MOTION Z ID, motion
Parameters
    ID
Integer identification number of the joint
    motion
Integer there are 3 possible values for this parameter, 0 will lock the joint and not allow relative motion, 1 wil only allow motion within a specified range while 2 will give the joint a full range of motions
Returns
Example Code

    No example code is provided for this command