TNL AVAILABLE This command will return a value of one if the current device uses hardware TNL.
Syntax
    Return Integer=TNL AVAILABLE()
Returns
This command will return a value of one if the current device uses hardware TNL. TNL stands for Transformation and Lighting
Description
TNL stands for Transformation and Lighting. Most cards these days support TNL in hardware as standard.
Example Code
    backdrop off : cls : sync on : sync rate 0 : hide mouse:cls 0

    ObjectNumber=1

    load object "models\model.x",ObjectNumber

    print "MISC"

    print "alphablending available:";alphablending available()

    print "filtering available:";filtering available()

    print "fog available:";fog available()

    print "TnL available:";tnl available()

    print "Polys on nscreen:";statistic(1)

    while mouseclick()=0

    sync

    endwhile

    while mouseclick()=1:endwhile

    delete object ObjectNumber

    end
See also
BASIC3D Commands Menu Index