PHY SET 6DOF JOINT GLOBAL AXIS Set the global axis.
Syntax
    PHY SET 6DOF JOINT GLOBAL AXIS ID, index, x#, y#, z#
Parameters
    ID
Integer identification number of the joint
    index
Integer the index of the rigid body that is attached to the joint that is to have its global anchor modified, this can either be 0 or 1
    x#
Float direction on the X axis
    y#
Float direction on the Y axis
    z#
Float direction on the Z axis
Returns
Description
This command will set the global axis for the specified rigid body attached to the 6DOF joint.
Example Code

    No example code is provided for this command