SET POINT LIGHT This command will set an existing light to that of a point light.
Syntax
    SET POINT LIGHT Light Number, X, Y, Z
Parameters
    Light Number
Integer The light number
    X
Float The x position is specified using a coordinate in 3D space
    Y
Float The y position is specified using a coordinate in 3D space
    Z
Float The z position is specified using a coordinate in 3D space
Returns
This command does not return a value.
Description
The position is specified using a coordinate in 3D space. The light number must be specified using an integer value. The coordinate must be specified using real values.
Example Code
    sync on

    autocam off

    color backdrop rgb(0,0,0)

    load image "ground.jpg",1

    make matrix 1,1000,1000,100,100

    prepare matrix texture 1,1,1,1

    position matrix 1,-500,0,-500

    position camera 0,100,0

    set ambient light 20

    color ambient light rgb(64,64,128)

    set point light 0,0,0,500

    position light 0,0,100,0

    color light 0,512,512,255

    set light range 0,1000

    while inkey$()<>"x"

    set cursor 0,0

    print "LIGHT COMMANDS (X to Exit)"

    sync

    endwhile

    end
See also
LIGHT Commands Menu Index