GET BACKBUFFER PTR This command will return the actual pointer to the backbuffer.
Syntax
    Return Integer=GET BACKBUFFER PTR()
Returns
A memory pointer to the backbuffer
Description
You can pass the pointer to a DLL which can directly access the memory of the backbuffer. You can only use this command when you have used the LOCK BACKBUFFER command.
Example Code
    cls

    set display mode 800,600,32

    wait 1000*8

    print "backbuffer pointer "+str$(get backbuffer ptr())

    do

    loop

    end
See also
DISPLAY Commands Menu Index